	Proposal Number
	Organization
	Paragraph                                                           / subpara / PG#
	Figure / Table / line #
	Comment Type           ( G / T / E )
	Comment
	Proposed Change
	Fixed Y/N

	1 
	Carl Anderson 
	112-113
	2.3.1.1
	T
	Clearly make Address ID mandatory 
	Clearly make Address ID mandatory by creating a grid indicating the Mandatory/Conditional/Optional status of each Simple Element 
	

	2 
	US Census Bureau 
	
	
	T
	Allow Geometry to be multiple.  Provide clear means of stating what the coordinates represent (position).
	 Add Map Position element and Address Position (child) element.
	

	3 
	Carl Anderson 
	483
	
	T
	Add a table indicating the Mandatory/Conditional/Optional status of each Element 
	Insert a column in the table in Appendix C called Obligation (Mandatory or Optional) 
	

	4 
	Carl Anderson 
	
	
	T
	Add Conformance levels/definitions and test for each level 
	
	

	5 
	US Census Bureau 
	
	
	T
	Correct XML schema issues as identified in attached spreadsheet 
	  
	

	6 
	Carl Anderson 
	
	
	T
	Add a definition of a JSON encoding of the transfer model 
	  
	

	7 
	US Census Bureau 
	
	
	T
	Add Feature Type core codelist  Feature Type notes and examples are a mix of objects and positions.
	Update notes and examples to better reflect common feature types such as parcel, building, residential house, apartment complex, unit, intersection, etc.
	

	8 
	US Census Bureau 
	
	
	T
	Add Position Type core codelist 
	  
	

	9 
	US Census Bureau 
	
	
	T
	Add a Feature Type subType or Heirarchy 
	  
	

	10 
	US Census Bureau 
	
	
	G
	Add a Feature Type repository authority (following ISO19110) 
	  
	

	11 
	US Census Bureau 
	506
	Appendix I: 2.2.2
	G
	Add more explicit examples of linking to NSDI Cadastral Standard 
	  
	

	12 
	US Census Bureau 
	510
	Appendix I: 2.8.2
	G
	Add more explicit examples of linking to NSDI Transportation Standard 
	  
	

	13 
	US Census Bureau 
	416
	
	T
	Indicate that Address ID element should be mandatory. 
	Insert the following sentence into the xsd:documentation documentation element after the last sentence: “Every address shall have an Address Id. 
	y

	14 
	US Census Bureau 
	464
	
	T
	Modify the schema to make the Address ID element mandatory 
	Remove the Address Id element from the Address Attributes_group. This is suggested in order to make the Address Id element mandatory. 
	y

	15 
	US Census Bureau 
	468
	
	T
	Make the Address Id element mandatory for the Numbered Thoroughfare Address_type. 
	Insert the following into the into the Numbered Thoroughfare Address_type: <xsd:element name=""AddressId"" type=""addr_type: Address ID_type"/>. This change is suggested to make the Address ID mandatory. 
	y

	16 
	US Census Bureau 
	469
	
	T
	Make the Address Id element mandatory for the Intersection Address_type 
	insert the following into the Intersection Address_type: <xsd:element name=""AddressId"" type=""addr_type:AddressID_type" 
	y

	17 
	US Census Bureau 
	469
	
	T
	Make the Address Id element man1datory for the Two Number Address Range class 
	insert the following into the ITwo Number Address Range_type: <xsd:element name="AddressId" type="addr_type:AddressID_type 
	y

	18 
	US Census Bureau 
	470
	
	T
	Make the Address Id mandatory for the Four Number Address Range 
	insert the following into the Four Number Address Range_type: <xsd:element name="AddressId" type="addr_type:AddressID_type" 
	y

	19 
	US Census Bureau 
	471
	
	T
	Make the Address Id mandatory for the Unnumbered Thoroughfare Address Class 
	insert the following into the into the Unnumbered Thoroughfare Address Type: <xsd:element name="AddressId" type="addr_type:AddressID_type"/> 
	y

	20 
	US Census Bureau 
	472
	
	T
	Make the Address Id mandatory for the Landmark Address class 
	insert the following into the Landmark Address class: <xsd:element name="AddressId" type="addr_type:AddressID_type"/> 
	y

	21 
	US Census Bureau 
	472
	
	T
	Make the Address Id element mandatory for the Community Address class 
	insert the following into the Community Address_type: <xsd:element name="AddressId" type="addr_type:AddressID_type"/> 
	y

	22 
	US Census Bureau 
	473
	
	T
	Make the Address Id element mandatory for the USPS Postal Delivery Route class 
	insert the following into the USPS Postal Delivery Route_type: <xsd:element name="AddressId" type="addr_type:AddressID_type"/> 
	y

	23 
	US Census Bureau 
	473
	
	T
	Make the Address Id mandatory for the USPS General Delivery Office class 
	insert the following into the USPS General Delivery Office type: <xsd:element name="AddressId" type="addr_type:AddressID_type"/> 
	y

	24 
	US Census Bureau 
	474
	
	T
	Make the Address Id mandatory for the General Address Class 
	"insert the following into the General Address Class type: <xsd:element name="AddressId" type="addr_type:AddressID_type"/>" 
	Y

	25 
	US Census Bureau 
	392
	First comment on the page (indicated by <!-- )
	T
	Change the version to 2.0
	change “0.4.3” to “2.0” 
	Y

	26 
	US Census Bureau 
	392
	Second comment on the page (indicated by <!-- )
	T
	Change the version to 2.0
	change “0.4.3” to “2.0” 
	y

	27 
	US Census Bureau 
	392
	The version_type simple type
	T
	Change the version to 2.0
	change <xsd:enumeration value='0.4.3' /> to <xsd:enumeration value=2.0 /> 
	y

	28 
	US Census Bureau 
	467
	First comment on the page (indicated by <!-- )
	T
	Change the version to 2.0
	change “0.4.3” to “2.0” 
	y

	29 
	US Census Bureau 
	467
	Second comment on the page (indicated by <!-- )
	T
	Change the version to 2.0
	change “0.4.3” to “2.0” 
	y

	30 
	US Census Bureau 
	476
	Numbered Thoroughfare Address
	T
	Change the version to 2.0 by changing the version attribute of the Address Collection element 
	change version="0.4" to version="2.0" 
	y

	31 
	US Census Bureau 
	476
	Numbered Thoroughfare Address
	T
	Make the Address Id element mandatory for the Numbered Thoroughfare Address_type. 
	Insert the Address Id element in the example. 
	y

	32 
	US Census Bureau 
	476
	Intersection Address
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="2.0" 
	y

	33 
	US Census Bureau 
	476
	Intersection Address
	T
	Make the Address Id element mandatory for the Intersection Address Address_type. 
	Insert the Address Id element in the example. 
	y

	34 
	US Census Bureau 
	477
	Two Number Address Range
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	35 
	US Census Bureau 
	477
	Two Number Address Range
	T
	Make the Address Id element mandatory for the Two Number Address Range. 
	Insert the Address Id element in the example. 
	y

	36 
	US Census Bureau 
	477
	Four Number Address Range
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	37 
	US Census Bureau 
	477
	Four Number Address Range
	T
	Make the Address Id element mandatory for the Four Number Address Range. 
	Insert the Address Id element in the example. 
	y

	38 
	US Census Bureau 
	478
	Unnumbered Thoroughfare Address
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	39 
	US Census Bureau 
	478
	Landmark Address
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element. 
	change version="0.4" to version="0.4.4" 
	y

	40 
	US Census Bureau 
	478-479
	Landmark Address
	T
	Make the Address Id element mandatory for the Landmark Address. 
	Insert the Address Id element in the example. 
	y

	41 
	US Census Bureau 
	478
	Unnumbered Thoroughfare Address
	T
	Make the Address Id element mandatory for the Unnumbered Thoroughfare Address 
	Insert the Address Id element in the example. 
	y

	42 
	US Census Bureau 
	479
	Community Address
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	43 
	US Census Bureau 
	479
	Community Address
	T
	Make the Address Id element mandatory for the Community Address 
	Insert the Address Id element in the example. 
	y

	44 
	US Census Bureau 
	480
	USPS Postal Delivery Box
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	45 
	US Census Bureau 
	480
	USPS Postal Delivery Box
	T
	Make the Address Id element mandatory for the USPS Postal Delivery Box 
	Insert the Address Id element in the example. 
	y

	46 
	US Census Bureau 
	480
	USPS Postal Delivery Route
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	47 
	US Census Bureau 
	480
	USPS Postal Delivery Route
	T
	Make the Address Id element mandatory for the USPS Postal Delivery Route 
	Insert the Address Id element in the example. 
	y

	48 
	US Census Bureau 
	481
	USPS General Delivery Office
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	49 
	US Census Bureau 
	481
	USPS General Delivery Office
	T
	Make the Address Id element mandatory for the USPS General Delivery Office 
	Insert the Address Id element in the example. 
	y

	50 
	US Census Bureau 
	481
	General Address Type 1
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	51 
	US Census Bureau 
	481
	General Address Type 1
	T
	Make the Address Id element mandatory for the General Address Type 1 
	Insert the Address Id element in the example. 
	y

	52 
	US Census Bureau 
	481
	General Address Type 2
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	53 
	US Census Bureau 
	481
	General Address Type 2
	T
	Make the Address Id element mandatory for the General Address Type 2 class 
	Insert the Address Id element in the example. 
	y

	54 
	US Census Bureau 
	482
	General Address Type 3
	T
	Change the version to 2.0by changing the version attribute of the Address Collection element 
	change version="0.4" to version="0.4.4" 
	y

	55 
	US Census Bureau 
	482
	General Address Type 3
	T
	Make the Address Id element mandatory for the General Address Type 3 
	Insert the Address Id element in the example. 
	y

	56 
	US Census Bureau 
	125
	2.3.2.6
	G
	Add the Unit Of Measure attribute to the Address Elevation element to indicate what unit was used to measure the Address Elevation. 
	Add the Unit Of Measure attribute to the Address Elevation 
	

	57 
	US Census Bureau 
	231
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	58 
	US Census Bureau 
	234
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	59 
	US Census Bureau 
	237
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	60 
	US Census Bureau 
	240
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	61 
	US Census Bureau 
	243
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	62 
	US Census Bureau 
	245
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	Y

	63 
	US Census Bureau 
	247
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	64 
	US Census Bureau 
	250
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	65 
	US Census Bureau 
	254
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	66 
	US Census Bureau 
	257
	
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	67 
	US Census Bureau 
	259
	Type 2
	T
	Change the version to 2.0
	change "0.4.2" to "0.4" 
	y

	68 
	US Census Bureau 
	259
	Type 3
	T
	Change the version to 2.0
	change "0.4.2" to "0.4.4" 
	y

	69 
	US Census Bureau 
	420-421
	Address Reference System Grid Angle_type
	T
	Change the Address Reference System Grid Angle_type from a complexType to a simpleType 
	Replace the current Address Reference System Grid Angle_type complex type with the following: <xsd:simpleType name="AddressReferenceSystemGridAngle_type"> <xsd:annotation> <xsd:documentation xml:lang="en">The degree to which a specific, named address grid is tilted off a north/south or east/west orientation. </xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:double"> </xsd:restriction> 
</xsd:simpleType> 
	[bookmark: _GoBack]y

	70 
	US Census Bureau 
	
	
	T
	Add a Sub Country Code 
	To be compatible with ISO 3166-2 
	

	71 
	Ed Wells 
	Part 2 all
	
	G
	Framework Data Content Standard requires that element descriptions include min/max occurrences. It is now shown only in XSD 
	Add min/max occurs to each element description. Make explicit what is in the XSD. 
	

	72 
	Ed Wells 
	Part 2 all
	
	T
	Framework Data Content Standard requires that element descriptions include conditionality. It is now shown only in XSD 
	Add conditionality to each element description (mandatory, conditional-mandatory, conditional-optional, optional). Make explicit what is in the XSD. 
	

	73 
	Ed Wells 
	
	
	T
	The address authority is not always the same as the address ID assigner. Examples: address aggregators; postal address compilers, etc. .Create address databases but do not assign addresses. 
	Add new element: Address IDAssigner. This will tell data users the source of the Address ID 
	

	74 
	Ed Wells 
	
	
	T
	"Pre" and "Post" are prefixes not words. 
	change English language representation of pre and post street name elements 
	

	75 
	Ed Wells 
	
	
	T
	"Street Name" is confusing as an element name, because the phrase typically refers to the Complete Street Name. 
	Rename Street Name element "Street Name Base" or something similar. 
	

	76 
	Ed Wells 
	
	
	T
	Separator element is logically three distinct elements that do three different things. 
	Split Separator element into three different elements (pretype, range, intersection) and rename. 
	

	77 
	Ed Wells 
	
	
	T
	Address Standard provides no way to show which side of a limited access highway is referenced. This matters for 9-1-1 responders. 
	Allow "southbound" "northbound" "eastbound" "westbound" (uncapitalized) as Street Name Postmodifiers 
	

	78 
	Ed Wells 
	
	
	T
	How to parse service road names such as "Lee Highway Access Road" or "Industrial Parkway Frontage Road"? 
	Add a note to the relevant element descriptions. 
	

	79 
	Martha Wells 
	
	
	T
	Standard provides no way to construct or parse highway interchange ramp names ("I-95 North to I-270 East Ramp"). These matter to 9-1-1 responders and road maintenance workers. 
	Research and define a syntax or class for highway interchange ramps. Functionally they are turn movements within an intersection, so they might be considered an extension of the Intersection Class. Are any new elements needed to construct the names? 
	

	80 
	Ed Wells 
	
	
	T
	Place name notes do not distinguish legislative, administrative, and unofficial place names 
	Revise place name notes along the lines of the CLDXF discussion. 
	

	81 
	Ed Wells 
	
	
	T
	Address ID should be required only for systems of address records (i.e. where the address is expected to be unique). Not required where address is embedded in some other record system (e.g. 9-1-1 calls, Social Security recipients) where addresses may be repeated. 
	Revise notes to clarify when Address ID is required. This is necessary for some profiles. 
	

	82 
	Ed Wells 
	
	
	T
	Add Street Name ID to distinguish unique street names in support of a master street name list. 
	Complete Street Name ID 
	

	83 
	Ed Wells 
	
	
	T
	Should critical address elements have start and end dates to show lifecycle status? 
	Consider adding start and end dates for address Number, street name, place name, zip? 
	

	84 
	Ed Wells 
	
	
	G
	Address Standard and Framework Transportation Standard conflict on certain points (e.g. street name elements) 
	Reconcile address standard with transportation Standard. May lead to changes in Framework Transportation Standard. 
	

	85 
	Ed Wells 
	
	
	T
	USPS Pub 28 is now in v2014 
	Review Postal Profile for changes 
	

	86 
	Ed Wells 
	
	
	T
	NENA CLDXF has changed substantially since 2011 and has been adopted soon. FGDC-CLDXF has been revised accordingly in that standard. 
	Replace v2011 provisional profile with v2013 CLDXF profile. Maintain in parallel with changes to relevant FGDC elements. 
	

	87 
	Mass GIS 
	
	
	T
	The standard does not provide enough guidance on the distinction between landmark addresses for buildings and addresses that would be have a sub-address type of building and a sub-address identifier. Is any named building on a campus a landmark?
	Add to the notes / comments for both these elements.
	

	88 
	Mass GIS 
	
	
	T
	Having the subaddress type be free-form, and leaving the domain to local authorities, seems too loose. 
	Consider having a domain for this element. 
	

	89 
	Fairview Industries 
	
	
	G
	Define roles and use consistently throughout, for example, producers (assigners, authoritative source), aggregators (compilers), publishers (trusted source, api etc.) 
	  
	

	90 
	Fairview Industries 
	
	
	G
	Define an essential core data set that could be used by perhaps smaller or less sophisticated jurisdictions 
	  
	

	91 
	Sara Yurman 
	
	
	
	  
	  
	

	92 
	US Census Bureau 
	360
	Section 5.2
	G
	Replace FGDC Content Standard for Digital Geospatial Metadata (CSDGM) with the ISO 19115-1 Standard. The FGDC CSDGM is being phased out. 
	Change the FGDC CSDGM part of the exchange with ISO Standard 19115-1 
	

	93 
	Census 
	259
	
	T
	Change the Example for the General Address Type 1 to an XML example
	Make it an XML example
	y

	94 
	Census 
	31
	
	G
	Add a definition for the Action attribute to the address class
	Add a definition for the Action attribute to the address class 
	

	95 
	Census 
	186
	After 2.3.9.4
	E
	
	Insert a definition for the action element of each address class. This attribute exists for each address class in the schema but the text of the standard makes no mention of it. 
	

	96 
	US Census Bureau 
	185
	2.3.9.4
	T
	Add schema for this element (Address Direct Source). Decide where this should go in the address class 
	Add a schema and an XML element for this element. 
	

	97 
	US Census Bureau 
	214
	2.5.16
	E
	The name of the Address Reference System Reference Polyline element needs to be corrected. The XML example needs to be updated to reflect GML 3.2.1 
	Change the name of the element name from Address Reference System Reference Polyline to Address Reference System Reference Polyline. Fix the XML example by supplying gml:id for the gml:MultiCurve and gml:Curve elements. 
	y

	98 
	US Census Bureau 
	216
	2.5.17
	E/T
	The schema and the XML example for the Address Reference System Range Breakpoint element needs to be corrected. 
	Correct the schema and XML example for the Address Reference System Range Breakpoint element. 
	

	99 
	US Census Bureau 
	218
	2.5.18
	T/E
	Correct the name for the Address Reference System Range Breakline element. 
	Fix the schema and XML example to reflect GML 3.2.1. 
	

	100 
	US Census Bureau 
	198
	2.5.4
	T/E
	Correct the schema and the XML example to reflect GML 3.2.1 for the Address Reference System Extent element 
	Correct the schema and XML example. 
	

	101 
	US Census Bureau 
	212
	2.5.14
	T/E
	Correct the schema and XML example to reflect GML 3.2.1 for the Address Reference System Axis Point Of Beginning element. 
	  
	

	102 
	US Census Bureau 
	222
	2.5.21
	T/E
	Correct the schema for "AddressReferenceSystem 
	  
	

	103 
	US Census Bureau 
	210
	2.5.13
	T/E
	Correct the schema for the Address Reference System Axis. Also update the XML example to reflect GML 3.2.1. 
	  
	

	104 
	US Census Bureau 
	219
	2.5.19
	T/E
	Correct the XML schema and update the XML example to reflect GML 3.2.1. Also confirm its order in the Address Reference System_type and its multiplicity. 
	  
	

	105 
	US Census Bureau 
	222
	2.5.21
	T/E
	Update the schema for the Address Reference System to reflect the updates made to the schemas for the other Address Reference System elements 
	  
	



