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[image: ]As a part of the U.S. Census Bureau's Geographic Support System Initiative (GSS-I), the Census Bureau is committed to accepting data from our partners beginning in fiscal year 2013.  The following tables list the metadata elements that are optimum for providing the Census Bureau with the information it needs to use partner data. The elements in the tables describe information about the entity responsible for the maintenance of  feature and/or  the address information, use restrictions, data lineage information, known data defects and a description of the geographic area the data represents.  September 6, 2012 v0.5


Note that commonly used projection elements are shown in the table. If you use a different projection than those listed, please provide the specific parameters in accordance with the Federal Geographic Data Committee (FGDC) Content Standard for Digital Geospatial Metadata (CSDGM), which can be found at http://www.fgdc.gov/metadata.

 Metadata editors can be found at: http://www.fgdc.gov/metadata/geospatial-metadata-tools.

FGDC Document Referenced
Document Number 	Document Name
FGDC-STD-001-1998	Content Standard for Digital Geospatial Metadata (CSDGM)

Identification Information
	Element and Description
	CSDGM 
Short Name
	CSDGM Element #

	Citation Information
	
	

	Originator (The name of the organization that developed the product)
	origin
	8.1

	Publication Date (The date the address and/or feature  data was released)
	pubdate
	8.2

	Title (The name of the address and/or feature product being released)
	title
	8.4

	Description
	
	

	Abstract (A brief summary of the product)
	abstract
	1.2.1

	Purpose (Reason why the data was developed)
	purpose
	1.2.2

	Time Period of Content
	
	

	Beginning Date (The start date of the period the addresses and/or features cover)
	begdate
	9.3.1

	Ending Date (The end date of the period the addresses and/or features cover)
	enddate
	9.3.3

	Currentness Reference (Basis on which the Beginning Date and Ending Date are  determined )
	current
	1.3.1

	Status
	
	

	Progress (The state of the product. It can either be “Complete”, “In work” or “planned”)
	progress
	1.4.1

	Maintenance and Update Frequency (The frequency with which changes and additions are made to  the data)
	update
	1.4.2

	Bounding Coordinates
	
	

	West Bounding Coordinate (The western most coordinate of coverage in decimal degrees)

	westbc
	1.5.1.1

	[bookmark: _GoBack]East Bounding Coordinate(The eastern most coordinate of coverage in decimal degrees)
	eastbc
	1.5.1.2

	North Bounding Coordinate (The northern most coordinate of coverage in decimal degrees)
	northbc
	1.5.1.3

	South Bounding Coordinate (The southernmost coordinate of coverage in decimal degrees)
	southbc
	1.5.1.4

	Theme Keywords
	
	

	Theme Keyword Thesaurus (A reference to a formally registered thesaurus. If none is used, the value is “none”)
	themekt
	1.6.1.1

	Theme Keyword (A common-use word or phrase to describe the product. An example would be “address”)
	themekey
	1.6.1.2

	Place Keywords
	
	

	Place Keyword Thesaurus (A reference to a formally registered thesaurus. If none is used, the value is “none”)
	placekt
	1.6.2.1

	Place Keyword (The geographic name of a location described by the product)
	placekey
	1.6.2.2

	Constraints
	
	

	Access Constraints (Any legal restrictions on accessing the product)
	accconst
	1.7

	Use Constraints (Any legal restrictions on using the product)
	useconst
	1.8







Data Quality Information
	Element and Description
	CSDGM       Short Name
	CSDGM Element #

	Quality Reports
	
	

	Logical Consistency Report (Details of the tests performed on the address and/or feature  data)
	logic
	2.2

	Completeness Report (information about omissions, selection criteria used to develop address and/or feature data) 
	complete
	2.3

	Process Steps
	
	

	Process Description (An explanation of how the address and/or feature data was processed)
	procdesc
	2.5.2.1

	Process Date (The date the process described under Process Description was completed)
	procdate
	2.5.2.3



Entity and Attribute Information
	Element and Description
	CSDGM     Short Name
	CSDGM Element #

	Entity and Attribute Overview (A detailed summary of the entity types, attributes and values in the address and/or feature file)
	eaover
	5.2.1

	Entity and Attribute Detail Citation (A reference to the complete description of the entity types and values) 
	eadetcit
	5.2.2



Contact Information
	Element and Description
	CSDGM  Short Name
	CSDGM Element #

	Contact Organization (The name of the organization that is responsible for the product)
	cntorg
	10.2.1

	Address Type (The type of address described by the Address element. This is usually ‘mailing’)
	addrtype
	10.4.1

	Address (The  street address of the organization that is responsible for the product)
	address
	10.4.2

	City (The city the organization that is responsible for the product is located in)
	city
	10.4.3

	State or Province (The state the organization that is responsible for the product is located in)
	state
	10.4.4

	Postal Code (The ZIP code of the organization that is responsible for the product)
	postal
	10.4.5

	Contact Voice Telephone (The voice telephone number for the organization that is responsible for the product)
	cntvoice
	10.5

	Contact Facsimile Telephone (The fax number for the organization that is responsible for the product)
	cntfax
	10.7

	Contact Electronic Mail Address (The email address for the organization that is responsible for the product)
	cntemail
	10.8



Metadata Information
	Element and Description
	CSDGM  Short Name
	CSDGM Element #

	Metadata Date (The date the metadata file was created)
	metd
	7.1

	Metadata Standard Name ( always Content Standard for Digital Geospatial Metadata)
	metstdn
	7.5

	Metadata Standard Version (always FGDC-STD-001-1998)
	metstdv
	7.6




Spatial Reference Information for unprojected coordinates
	Element and Description
	CSDGM  Short Name
	CSDGM Element #

	Geographic
	
	

	Latitude Resolution (The minimum difference between two adjacent latitude values in Geographic Coordinate Units expressed in coordinate units of measure)
	latres
	4.1.1.1

	Longitude Resolution (The difference between two adjacent longitude values in Geographic Coordinate Units expressed in coordinate units of measure)
	longres
	4.1.1.2

	Geographic Coordinate Units (Units used for the Latitude Resolution and Longitude Resolution elements)
	geogunit
	4.1.1.3

	Geodetic Model
	
	

	Horizontal Datum Name (Either “North American Datum of 1927” or “North American Datum of 1983”)
	horizdn
	4.1.4.1

	Ellipsoid Name (Either “Clarke 1866” or “Geodetic Reference System 80”)
	ellips
	4.1.4.2

	Semi-Major Axis (The radius of the equatorial axis of the ellipsoid in meters)
	semiaxis
	4.1.4.3

	Denominator of Flattening Ratio (The denominator of the ratio of difference between the equatorial and polar radii)
	denflat
	4.1.4.4




Spatial Reference Information for State Plane Coordinates using a Lambert Conformal Conic projection
	Element and Description
	CSDGM  Short Name
	CSDGM Element #

	Planar / Grid Coordinate System / State Plane Coordinate System / Lambert Conformal Conic

	Grid Coordinate System Name (Either “State Plane Coordinate System 1927”,   or “State Plane Coordinate System 1983”)
	gridsysn
	4.1.2.2.1

	SPCS Zone Identifier (Identifier for the State Plane Coordinate System zone)
	spcszone
	4.1.2.2.4.1

	Standard Parallel (A line of constant latitude, expressed in decimal degrees, at which the surface of the Earth and the plane intersect. This may be used 1 or 2 times)
	stdparll
	4.1.2.1.23.1

	Standard Parallel (A line of constant latitude, expressed in decimal degrees, at which the surface of the Earth and the plane intersect)
	stdparll
	4.1.2.1.23.1

	Longitude of Central Meridian (The line of longitude at the center of the Lambert Conformal Conic Projection in decimal degrees)
	longcm
	4.1.2.1.23.2

	Latitude of Projection Origin (The latitude chosen as the origin of the coordinates for the map projection)
	latprjo
	4.1.2.1.23.3

	False Easting (The value added to all “x” values in the coordinates for a map projection)
	feast
	4.1.2.1.23.4

	False Northing (The value added to all “y” values in the coordinates for a map projection)
	fnorth
	4.1.2.1.23.5

	Planar Coordinate Information
	
	

	Planar Coordinate Encoding Method (Method used to represent horizontal positions within the coordinate system.  Either “coordinate pair”, distance and bearing” or “row and column”)
	plance
	4.1.2.4.1

	Abscissa Resolution (The minimum distance between “X” values of two adjacent points in the planar data set This is the “fuzzy tolerance”) 
	abusers
	4.1.2.4.2.1

	Ordinate Resolution (The minimum distance between “Y” values of two adjacent points in the planar data set This is the “fuzzy tolerance”)
	ordres
	4.1.2.4.2.2

	Planar Distance Units (The units of measure used to define the Coordinate Resolution)
	plandu
	4.1.2.4.4

	Geodetic Model
	
	

	Horizontal Datum Name (Either “North American Datum of 1927” or North American Datum of 1983”)
	horizdn
	4.1.4.1

	Ellipsoid Name (Either “Clarke 1866” or “Geodetic Reference System 80”)
	ellips
	4.1.4.2

	Semi-Major Axis (The radius of the equatorial axis expressed in meters)
	semiaxis
	4.1.4.3

	Denominator of Flattening Ratio (The denominator of the ratio of difference between the equatorial and polar radii)
	denflat
	4.1.4.4




Spatial Reference Information for State Plane Coordinates using a Transverse Mercator projection
	Element and Description
	CSDGM 
Short Name
	CSDGM Element #

	Planar / Grid Coordinate System / State Plane Coordinate System / Transverse Mercator

	Grid Coordinate System Name (“Universal Transverse Mercator”)
	gridsysn
	4.1.2.2.1

	SPCS Zone Identifier (Identifier for the State Plane Coordinate System zone)
	spcszone
	4.1.2.2.4.1

	Scale Factor at Central Meridian (a multiplier for reducing a distance obtained from a map by computation or scaling to the actual distance along the central meridian)
	sfctrmer
	4.1.2.1.23.17

	Longitude of Central Meridian (The line of longitude at the center of the Lambert Conformal Conic Projection in decimal degrees)
	longcm
	4.1.2.1.23.2

	Latitude of Projection_Origin (The latitude chosen as the origin of the coordinates for the map projection)
	latprjo
	4.1.2.1.23.3

	False Easting (The value added to all “x” values in the coordinates for a map projection)
	feast
	4.1.2.1.23.4

	False Northing (The value added to all “y” values in the coordinates for a map projection)
	fnorth
	4.1.2.1.23.5

	Planar Coordinate Information
	
	

	Planar Coordinate Encoding Method (Either “coordinage pair”, “distance and bearing” or “row and column”)
	plance
	4.1.2.4.1

	Abscissa Resolution (The minimum distance between “X” values of two adjacent points in the planar data set This is the “fuzzy tolerance”)
	absres
	4.1.2.4.2.1

	Ordinate Resolution (The minimum distance between “Y” values of two adjacent points in the planar data set This is the “fuzzy tolerance”)
	ordres
	4.1.2.4.2.2

	Planar Distance Units (The units of measure used to define the Coordinate Resolution)
	plandu
	4.1.2.4.4

	Geodetic Model
	
	

	Horizontal Datum Name (Either “North American Datum of 1927” or North American Datum of 1983”)
	horizdn
	4.1.4.1

	Ellipsoid Name (Either “Clarke 1866” or “Geodetic Reference System 80”)
	ellips
	4.1.4.2

	Semi-Major Axis (The radius of the equatorial axis expressed in meters)
	semiaxis
	4.1.4.3

	Denominator of Flattening Ratio (The denominator of the ratio of difference between the equatorial and polar radii)
	denflat
	4.1.4.4
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