X. 2.2 Part 1: Cadastral 

X. 2.2.1. Scope of Part 1: Cadastral. 

Part 1 “provides the information necessary to identify the existence of parcel-level cadastral information and the source of that information.” (Part 1, Sec. 1). 

Part 1 is a profile of the FGDC's Cadastral Data Content Standard (FGDC-STD-003). The Cadastral Data Content Standard “contains the standardization of the definition of entities and objects related to cadastral information including survey measurements, transactions related to interests in land, general property descriptions, and boundary and corner evidence data.” (Part 1, Introduction). 

X. 2.2.2. Relation of Part 1 and the Cadastral Data Content Standard to the Address Standard. 

The address standard is unrelated to the Cadastral Part and to the Cadastral Data Content Standard. The address standard does not refer to parcels (except for the two attributes mentioned below), and it does not share any defined terms, data elements, or data classes with Part 1 or the Cadastral Data Content Standard. 

However, in practice parcel data and address data are closely related in many records, and the standards should also be related. 

The relation between addresses and parcels is anything but simple. There are addresses that locate features not on any parcel at all (e.g. large federal lands and public rights-of-way), on one parcel only, and on many parcels. Conversely there are parcels that have no address at all, parcels that have one address, and parcels that have many addresses (e.g. large parcels that front on more than one thoroughfare). Thus no specific address-parcel relationship can be assumed. Addresses and parcels should therefore be treated as independent of each other, and the relationship between should be treated, in relational database terms, as a many-to-many relationship. 

The address standard and the Cadastral Data Content Standard can support the establishment of address-parcel relationships by providing a standard structure for recording their relationships. By using a database linking or relationship table to relate Address ID with the Parcel Identifier as described in the Cadastral Data Content Standard, each address can be related to any number of parcels, and vice versa. 

The ASWG has therefore included two optional address attributes in the Data Content part, Address Parcel Identifier and Address Parcel Identifier Source, both defined by reference to the Cadastral Data Content Standard. 

X.2.2.3. Recommendation from the ASWG to the FGDC SWG. 

That the maintenance authorities for Part 1 and for the Cadastral Data Content Standard confer with the ASWG to: 

1. Verify that the two optional address attributes in the Data Content part, Address Parcel Identifier and Address Parcel Identifier Source, are consistent with the Cadastral Data Content Standard. 

2. Add, within the Cadastral Data Content Standard, two corresponding attributes to the Parcel entity, Parcel Address ID and Parcel Address Authority, both to be defined by reference to the address standard. 
